[Profil]
rootx = [1.0, 1.0, 0.0, 0.0, 1.0]
rooty = [-0.943939, 0.943939, 0.943939, -0.943939, -0.943939]
roots = [4, 4.0, 4.0, 4.0, 4]
tipx = [1.0, 1.0, 0.0, 0.0, 1.0]
tipy = [-0.264848, 0.264848, 0.264848, -0.264848, -0.264848]
tips = [4, 4.0, 4.0, 4.0, 4]
nameroot = Rect1.dat
nametip = Rect2.dat

[Transform]
croot = 50.0
ctip = 100.0
cbcomplexprofiles = 1
incidenceroot = 0.0
thicknessroot = 100.0
tethicknessroot = 0.0
vinvertroot = 0
incidencetip = 0.0
thicknesstip = 100.0
tethicknesstip = 0.0
vinverttip = 0
covering = 0.0
smooth = 0
nbrpoints = 5
repartition = 1.0
reducepoints = 0

[Bloc]
bloclx = 350.0
blochz = 120.0
fleading = -25.0
ftrailing = 25.0
mleading = 10.0
mtrailing = 10.0
cbcutboth = 0
cbrotdelta = 0
rbleftwing = 1
rbrightwing = 0
rbtabletoblockleft = 1
rbtabletoblockright = 0
bloctotableleft = 100.0
bloctotableright = 110.0
bloctotabletrailingroot = 50.0
hoffset = 10.0
hprofileroot = 10.0
hprofiletip = 35.0
cbalignprofiles = 0
angleinroot = 0.0
angleintip = 0.0
angleoutroot = 0.0
angleouttip = 0.0
gbextracutcmdsactive = 1
extracutcommands = 

[Material]
mspeednorm = 2.0
mspeedhalf = 1.0
mspeedmin = 0.5
mspeedmax = 2.5
mradspnorm = 0.8
mradsphalf = 1.5
mheatspnorm = 80.0
mname = Yellow foam 40 kg/m3
mhotwire = NiCr, 800 mm x 0.3 mm, 24 V

[Table]
tableyy = 600.0
tableyg = 20.0
tableyd = 20.0
maxdiag = 750.0
cmaxy = 500.0
cmaxz = 400.0
vmaxy = 10.0
vmaxz = 5.0
theatingmax = 100.0
tname = My CNC
tcomport = Select port
tbaudrate = 115200
tpreheat = 5.0
tpostheat = 0.1
vcut = 2.0
gcodestart1 = 
gcodestart2 = 
gcodestart3 = 
gcodestart4 = 
gcodeend1 = 
gcodeend2 = 
gcodeend3 = 
gcodeend4 = 
gcodeletters = XYAZ

[Cut]
vcut = 2.0
vheat = 80.0
vusefoamparam = 1

[Guillotine]
gcuttingspeed = 2.0
gheating = 80.0
gusefoamparam = 1

